--------------------------------
loopy's PowerPak mapper set
--------------------------------

Copy to your POWERPAK\ folder:

MAP04.MAP:   MMC3 (mapper 4)
MAP13.MAP:   Namco-106 (mapper 19)
MAP15.MAP:   VRC4 (mapper 21)
MAP17.MAP:   VRC4 (mapper 23)
MAP19.MAP:   VRC4 (mapper 25)
MAP18.MAP:   VRC6 (mapper 24)
MAP45.MAP:   Sunsoft 5B (mapper 69)
F.MAP:       Famicom Disk System (FDS)
FDSBIOS.BIN: FDS system BIOS
M.MAP:       NSF mapper
NSF.NES:     NSF player rom


PowerPak mapper set 1.20 or later is required for FDS and NSF support.
Download from the RetroZone official website (retrousb.com)
To hear expansion audio, put a 47k resistor between pins 3 and 9 of the NES expansion connector.

--------------------------------
FDS
--------------------------------

Push any button on the FDS title screen to "insert" disk.
Disk side switching will happen automatically.
Hold the Select button to keep a disk ejected.
To save, hold reset for about 2 seconds, then choose a .FDS file to write to.

--------------------------------
NSF
--------------------------------

VRC6, FDS, and N106 expansion audio is supported.

L,R,B,A:   track select
up:        fast
down:      slow
start:     restart track
select:    return to PowerPak menu

--------------------------------
