Release 9.1i - par J.30
Copyright (c) 1995-2007 Xilinx, Inc.  All rights reserved.

Sat Jun 16 20:34:40 2007


INFO: The IO information is provided in three file formats as part of the Place and Route (PAR) process.  These formats are:
1. The <design name>_pad.txt file (this file) designed to provide information on IO usage in a human readable ASCII text format viewable through common text editors.
2. The <design namd>_pad.csv file for use with spreadsheet programs such as MS Excel. This file can also be read by PACE to communicate post PAR IO information.
3. The <design name>.pad file designed for parsing by customers.  It uses the "|" as a data field separator.

INPUT FILE:       map03_map.ncd
OUTPUT FILE:      map03_pad.txt
PART TYPE:        xc2s30
SPEED GRADE:      -5
PACKAGE:          tq144

Pinout by Pin Number:

+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
|Pin Number|Signal Name |Pin Usage|Pin Name    |Direction|IO Standard|IO Bank Number|Drive (mA)|Slew Rate|Termination|IOB Delay|Voltage|Constraint|DCI Value|IO Register|Signal Integrity|
+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
|P1        |            |         |VCCO        |         |           |0             |          |         |           |         |2.50   |          |         |           |                |
|P2        |            |         |TCK         |         |           |              |          |         |           |         |       |          |         |           |                |
|P3        |RAM_CHR_A13 |IOB      |IO          |TRISTATE |LVCMOS2    |0             |12*       |NONE*    |PULLUP     |         |       |LOCATED   |         |NO         |NONE            |
|P4        |RAM_CHR_A12 |IOB      |IO          |TRISTATE |LVCMOS2    |0             |12*       |NONE*    |PULLUP     |         |       |LOCATED   |         |NO         |NONE            |
|P5        |NES_CHR_A7  |IOB      |IO_VREF_0   |INPUT    |LVCMOS2    |0             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P6        |NES_CHR_A10 |IOB      |IO          |INPUT    |LVCMOS2    |0             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P7        |NES_CHR_A8  |IOB      |IO          |INPUT    |LVCMOS2    |0             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P8        |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P9        |            |         |VCCINT      |         |           |              |          |         |           |         |2.5    |          |         |           |                |
|P10       |NES_CHR_A11 |IOB      |IO          |INPUT    |LVCMOS2    |0             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P11       |RAM_CHR_A16 |IOB      |IO          |TRISTATE |LVCMOS2    |0             |12*       |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P12       |            |IOB      |IO_VREF_0   |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|P13       |RAM_CHR_A17 |IOB      |IO          |TRISTATE |LVCMOS2    |0             |12*       |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P14       |            |         |VCCINT      |         |           |              |          |         |           |         |2.5    |          |         |           |                |
|P15       |NES_CHR_RD  |GCLKIOB  |GCK3        |INPUT    |LVCMOS2    |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|P16       |            |         |VCCO        |         |           |0             |          |         |           |         |2.50   |          |         |           |                |
|P17       |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P18       |NES_M2      |GCLKIOB  |GCK2        |INPUT    |LVCMOS2    |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|P19       |            |IOB      |IO          |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|P20       |            |IOB      |IO          |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|P21       |RAM_CHR_A18 |IOB      |IO_VREF_1   |TRISTATE |LVCMOS2    |1             |12*       |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P22       |            |IOB      |IO          |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|P23       |            |IOB      |IO          |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|P24       |            |         |VCCINT      |         |           |              |          |         |           |         |2.5    |          |         |           |                |
|P25       |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P26       |RAM_CHR_CE  |IOB      |IO          |BIDIR    |LVCMOS2    |1             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P27       |            |IOB      |IO          |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|P28       |NES_PRG_A13 |IOB      |IO_VREF_1   |INPUT    |LVCMOS2    |1             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P29       |NES_CIRAM_CE|IOB      |IO          |BIDIR    |LVCMOS2    |1             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P30       |            |IOB      |IO_WRITE    |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|P31       |            |IOB      |IO_CS       |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|P32       |            |         |TDI         |         |           |              |          |         |           |         |       |          |         |           |                |
|P33       |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P34       |            |         |TDO         |         |           |              |          |         |           |         |       |          |         |           |                |
|P35       |            |         |VCCO        |         |           |0             |          |         |           |         |2.50   |          |         |           |                |
|P36       |            |         |VCCO        |         |           |1             |          |         |           |         |2.50   |          |         |           |                |
|P37       |            |         |CCLK        |         |           |              |          |         |           |         |       |          |         |           |                |
|P38       |RAM_PRG_D0  |IOB      |IO_DOUT_BUSY|BIDIR    |LVCMOS2    |2             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P39       |NES_PRG_D7  |IOB      |IO_DIN_D0   |BIDIR    |LVCMOS2    |2             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |YES        |NONE            |
|P40       |BOOT_ENABLE |IOB      |IO          |BIDIR    |LVCMOS2    |2             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P41       |            |IOB      |IO_VREF_2   |UNUSED   |           |2             |          |         |           |         |       |          |         |           |                |
|P42       |NES_PRG_A14 |IOB      |IO          |INPUT    |LVCMOS2    |2             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P43       |NES_IRQ     |IOB      |IO          |BIDIR    |LVCMOS2    |2             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P44       |NES_PRG_D6  |IOB      |IO_D1       |BIDIR    |LVCMOS2    |2             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |YES        |NONE            |
|P45       |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P46       |NES_PRG_D5  |IOB      |IO_D2       |BIDIR    |LVCMOS2    |2             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |YES        |NONE            |
|P47       |WRAM_PRG_WR |IOB      |IO          |BIDIR    |LVCMOS2    |2             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P48       |RAM_PRG_D1  |IOB      |IO_VREF_2   |BIDIR    |LVCMOS2    |2             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P49       |NES_PRG_D4  |IOB      |IO_D3       |BIDIR    |LVCMOS2    |2             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |YES        |NONE            |
|P50       |RAM_PRG_D3  |IOB      |IO          |BIDIR    |LVCMOS2    |2             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P51       |RAM_PRG_D4  |IOB      |IO_IRDY     |BIDIR    |LVCMOS2    |2             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P52       |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P53       |            |         |VCCO        |         |           |1             |          |         |           |         |2.50   |          |         |           |                |
|P54       |RAM_PRG_D5  |IOB      |IO_TRDY     |BIDIR    |LVCMOS2    |3             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P55       |            |         |VCCINT      |         |           |              |          |         |           |         |2.5    |          |         |           |                |
|P56       |RAM_PRG_D6  |IOB      |IO          |BIDIR    |LVCMOS2    |3             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P57       |NES_PRG_D3  |IOB      |IO_D4       |BIDIR    |LVCMOS2    |3             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |YES        |NONE            |
|P58       |RAM_PRG_D7  |IOB      |IO_VREF_3   |BIDIR    |LVCMOS2    |3             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P59       |NES_PRG_A10 |IOB      |IO          |INPUT    |LVCMOS2    |3             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P60       |NES_PRG_D2  |IOB      |IO_D5       |BIDIR    |LVCMOS2    |3             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |YES        |NONE            |
|P61       |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P62       |NES_PRG_D1  |IOB      |IO_D6       |BIDIR    |LVCMOS2    |3             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |YES        |NONE            |
|P63       |RAM_PRG_D2  |IOB      |IO          |BIDIR    |LVCMOS2    |3             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P64       |NES_PRG_A11 |IOB      |IO          |INPUT    |LVCMOS2    |3             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P65       |NES_PRG_A9  |IOB      |IO_VREF_3   |INPUT    |LVCMOS2    |3             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P66       |NES_PRG_A8  |IOB      |IO          |INPUT    |LVCMOS2    |3             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P67       |NES_PRG_D0  |IOB      |IO_D7       |BIDIR    |LVCMOS2    |3             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |YES        |NONE            |
|P68       |            |IOB      |IO_INIT     |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|P69       |            |         |PROGRAM     |         |           |              |          |         |           |         |       |          |         |           |                |
|P70       |            |         |VCCO        |         |           |1             |          |         |           |         |2.50   |          |         |           |                |
|P71       |            |         |VCCO        |         |           |2             |          |         |           |         |2.50   |          |         |           |                |
|P72       |            |         |DONE        |         |           |              |          |         |           |         |       |          |         |           |                |
|P73       |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P74       |NES_PRG_A3  |IOB      |IO          |INPUT    |LVCMOS2    |4             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P75       |RAM_PRG_WR  |IOB      |IO          |BIDIR    |LVCMOS2    |4             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P76       |NES_PRG_A2  |IOB      |IO          |INPUT    |LVCMOS2    |4             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P77       |NES_PRG_A1  |IOB      |IO_VREF_4   |INPUT    |LVCMOS2    |4             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P78       |NES_PRG_A0  |IOB      |IO          |INPUT    |LVCMOS2    |4             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P79       |NES_PRG_A12 |IOB      |IO          |INPUT    |LVCMOS2    |4             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P80       |WRAM_PRG_RD |IOB      |IO          |BIDIR    |LVCMOS2    |4             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P81       |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P82       |            |         |VCCINT      |         |           |              |          |         |           |         |2.5    |          |         |           |                |
|P83       |NES_PRG_A7  |IOB      |IO          |INPUT    |LVCMOS2    |4             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P84       |NES_PRG_A6  |IOB      |IO          |INPUT    |LVCMOS2    |4             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P85       |RAM_PRG_RD  |IOB      |IO_VREF_4   |BIDIR    |LVCMOS2    |4             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P86       |NES_PRG_A5  |IOB      |IO          |INPUT    |LVCMOS2    |4             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P87       |NES_PRG_A4  |IOB      |IO          |INPUT    |LVCMOS2    |4             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P88       |NES_CHR_WR  |GCLKIOB  |GCK0        |INPUT    |LVCMOS2    |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|P89       |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P90       |            |         |VCCO        |         |           |2             |          |         |           |         |2.50   |          |         |           |                |
|P91       |NES_CLK     |GCLKIOB  |GCK1        |INPUT    |LVCMOS2    |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|P92       |            |         |VCCINT      |         |           |              |          |         |           |         |2.5    |          |         |           |                |
|P93       |RAM_PRG_A13 |IOB      |IO          |TRISTATE |LVCMOS2    |5             |12*       |NONE*    |PULLUP     |         |       |LOCATED   |         |NO         |NONE            |
|P94       |            |IOB      |IO_VREF_5   |UNUSED   |           |5             |          |         |           |         |       |          |         |           |                |
|P95       |NES_PRG_RW  |IOB      |IO          |INPUT    |LVCMOS2    |5             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P96       |RAM_PRG_A14 |IOB      |IO          |TRISTATE |LVCMOS2    |5             |12*       |NONE*    |PULLUP     |         |       |LOCATED   |         |NO         |NONE            |
|P97       |            |         |VCCINT      |         |           |              |          |         |           |         |2.5    |          |         |           |                |
|P98       |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P99       |NES_PRG_CE  |IOB      |IO          |INPUT    |LVCMOS2    |5             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P100      |NES_CHR_A9  |IOB      |IO          |INPUT    |LVCMOS2    |5             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P101      |RAM_PRG_A17 |IOB      |IO          |TRISTATE |LVCMOS2    |5             |12*       |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P102      |RAM_PRG_A16 |IOB      |IO_VREF_5   |TRISTATE |LVCMOS2    |5             |12*       |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P103      |RAM_PRG_A15 |IOB      |IO          |TRISTATE |LVCMOS2    |5             |12*       |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P104      |            |         |NC          |         |           |              |          |         |           |         |       |          |         |           |                |
|P105      |            |         |NC          |         |           |              |          |         |           |         |       |          |         |           |                |
|P106      |            |         |M2          |         |           |              |          |         |           |         |       |          |         |           |                |
|P107      |            |         |VCCO        |         |           |2             |          |         |           |         |2.50   |          |         |           |                |
|P108      |            |         |VCCO        |         |           |3             |          |         |           |         |2.50   |          |         |           |                |
|P109      |            |         |M0          |         |           |              |          |         |           |         |       |          |         |           |                |
|P110      |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P111      |            |         |M1          |         |           |              |          |         |           |         |       |          |         |           |                |
|P112      |RAM_PRG_A18 |IOB      |IO          |TRISTATE |LVCMOS2    |6             |12*       |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P113      |NES_CHR_D1  |IOB      |IO          |BIDIR    |LVCMOS2    |6             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P114      |NES_CHR_D2  |IOB      |IO          |BIDIR    |LVCMOS2    |6             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P115      |NES_CHR_D4  |IOB      |IO_VREF_6   |BIDIR    |LVCMOS2    |6             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P116      |NES_CHR_D3  |IOB      |IO          |BIDIR    |LVCMOS2    |6             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P117      |RAM_CHR_A10 |IOB      |IO          |BIDIR    |LVCMOS2    |6             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P118      |RAM_CHR_A2  |IOB      |IO          |BIDIR    |LVCMOS2    |6             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P119      |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P120      |RAM_CHR_A1  |IOB      |IO          |BIDIR    |LVCMOS2    |6             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P121      |RAM_CHR_A11 |IOB      |IO          |BIDIR    |LVCMOS2    |6             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P122      |RAM_CHR_A0  |IOB      |IO_VREF_6   |BIDIR    |LVCMOS2    |6             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P123      |NES_CHR_D7  |IOB      |IO          |BIDIR    |LVCMOS2    |6             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P124      |RAM_CHR_A15 |IOB      |IO          |TRISTATE |LVCMOS2    |6             |12*       |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P125      |            |         |VCCINT      |         |           |              |          |         |           |         |2.5    |          |         |           |                |
|P126      |NES_CHR_A2  |IOB      |IO_TRDY     |INPUT    |LVCMOS2    |6             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P127      |            |         |VCCO        |         |           |3             |          |         |           |         |2.50   |          |         |           |                |
|P128      |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P129      |NES_CHR_D5  |IOB      |IO_IRDY     |BIDIR    |LVCMOS2    |7             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P130      |NES_CHR_A6  |IOB      |IO          |INPUT    |LVCMOS2    |7             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P131      |NES_CHR_A12 |IOB      |IO          |INPUT    |LVCMOS2    |7             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P132      |NES_CHR_A1  |IOB      |IO_VREF_7   |INPUT    |LVCMOS2    |7             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P133      |NES_CHR_D6  |IOB      |IO          |BIDIR    |LVCMOS2    |7             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P134      |RAM_CHR_A14 |IOB      |IO          |TRISTATE |LVCMOS2    |7             |12*       |NONE*    |PULLUP     |         |       |LOCATED   |         |NO         |NONE            |
|P135      |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P136      |NES_CHR_A5  |IOB      |IO          |INPUT    |LVCMOS2    |7             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P137      |NES_CHR_A0  |IOB      |IO          |INPUT    |LVCMOS2    |7             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P138      |NES_CHR_A13 |IOB      |IO          |INPUT    |LVCMOS2    |7             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P139      |NES_CHR_A3  |IOB      |IO_VREF_7   |INPUT    |LVCMOS2    |7             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P140      |NES_CHR_A4  |IOB      |IO          |INPUT    |LVCMOS2    |7             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P141      |NES_CHR_D0  |IOB      |IO          |BIDIR    |LVCMOS2    |7             |12*       |NONE*    |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|P142      |            |         |TMS         |         |           |              |          |         |           |         |       |          |         |           |                |
|P143      |            |         |GND         |         |           |              |          |         |           |         |       |          |         |           |                |
|P144      |            |         |VCCO        |         |           |3             |          |         |           |         |2.50   |          |         |           |                |
+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+

* Default value.
** This default Pullup/Pulldown value can be overridden in Bitgen. 
****** Special VCCO requirements may apply. Please consult the device 
       family datasheet for specific guideline on VCCO requirements. 


