CNROM Project Status
Project File: | cnrom.ise | Current State: | Programming File Generated
Module Name: | map03 | Errors: | No Errors
Target Device: | xc2s30-5tq144 | Warnings: | 130 Warnings (0 filtered)
Product Version: | ISE 9.1i | Updated: | Sat Jun 16 20:34:51 2007

CNROM Partition Summary
No partition information was found.

Device Utilization Summary
Logic Utilization | Used | Available | Utilization | Note(s)
Number of Slice Flip Flops | 204 | 864 | 23% |
Number of 4 input LUTs | 246 | 864 | 28% |
Logic Distribution |  |  |  |
Number of occupied Slices | 236 | 432 | 54% |
Number of Slices containing only related logic | 236 | 236 | 100% |
Number of Slices containing unrelated logic | 0 | 236 | 0% |
Total Number of 4 input LUTs | 246 | 864 | 28% |
Number of bonded IOBs | 81 | 92 | 88% |
IOB Flip Flops | 8 |  |  |
Number of Tbufs | 64 | 480 | 13% |
Number of Block RAMs | 4 | 6 | 66% |
Number of GCLKs | 1 | 4 | 25% |
Number of GCLKIOBs | 4 | 4 | 100% |
Number of RPM macros | 12 |  |  |
Total equivalent gate count for design | 69,074 |  |  |
Additional JTAG gate count for IOBs | 4,080 |  |  |

Performance Summary
Final Timing Score: | 0 | Pinout Data: | Pinout Report
Routing Results: | All Signals Completely Routed | Clock Data: | Clock Report
Timing Constraints: | All Constraints Met |  |

Detailed Reports
Report Name | Status | Generated | Errors | Warnings | Infos
Synthesis Report | Current | Sat Jun 16 20:34:22 2007 | 0 | 50 Warnings (0 filtered) | 0
Translation Report | Current | Sat Jun 16 20:34:28 2007 | 0 | 0 | 16 Infos (0 filtered)
Map Report | Current | Sat Jun 16 20:34:36 2007 | 0 | 52 Warnings (0 filtered) | 1 Info (0 filtered)
Place and Route Report | Current | Sat Jun 16 20:34:42 2007 | 0 | 14 Warnings (0 filtered) | 1 Info (0 filtered)
Static Timing Report | Current | Sat Jun 16 20:34:46 2007 | 0 | 14 Warnings (0 filtered) | 2 Infos (0 filtered)
Bitgen Report | Current | Sat Jun 16 20:34:52 2007 | 0 | 0 | 0